{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Zonas Seguras"],"read":"whole","date_system":"1900"}

{"sheet":"Zonas Seguras","index":0,"n_rows":105,"n_cols":6,"rows_kept":105,"merged":[[1,2,1,3],[2,2,2,3],[26,2,26,3],[49,2,49,3],[71,2,71,3],[85,2,85,3],[91,2,91,3],[95,2,95,3],[99,2,99,3],[100,2,100,3],[101,2,101,3],[102,2,102,3]]}
[]
[null,"ITEM","CONDICIONES TECNICAS MINIMAS ",null,"NO CUMPLE","CUMPLE"]
[null,1,"PTP Nodos Principales "]
[null,"1.1","Marca","Especificar"]
[null,"1.2","Modelo","Especificar"]
[null,"1.3","Cantidad","De acuerdo al cuadro de cantidades"]
[null,"1.4","Tipo ","Radio Capacidad Gigabit"]
[null,"1.5","Frecuencia & Duplexado","71-76GHz / 81-86GHz*, duplexado por división en frecuencia (FDD)"]
[null,"1.6","Canales","16/8/5/3 canales, anchos de canales 250/500/750/1250MHz"]
[null,"1.7","Modulación & tasa adaptiva","Hasta 5 niveles de velocidades sin errores por cambio.\nLa codificación y modulación adaptativa generan una ganacía de hasta 25dB"]
[null,"1.8","Capacidad","2Gbps, Full Duplex"]
[null,"1.9","Link budget (BER=10-6)","incluye ganancia de antena ½ft (podría no estar disponible en su región)\nincluye ganancia de antena 1ft\nincluye ganancia de antena 2f"]
[null,"1.10","Alcance (km)","2Gbps (zona de lluvia N con 99% disponibilidad, ant. 2ft.)\n2Gbps (zona de lluvia N con 99.99% disponibilidad, ant. 2ft.)\n1Gbps (zona de lluvia N con 99.99% disponibilidad, ant. 2ft.)"]
[null,"1.11","Puertos","4xGbE ports, (2x copper RJ-45 + 2x optical SFP SMF/MMF)"]
[null,"1.12","Características Ethernet","Puente transparente IEEE 802.1d\nVLAN & VLAN stacking, 4K VLANs\nServicios Ethernet que cumplen con la MEF 9, 14 y 21\nModo de puertos transparentes Smart Pipes\nAgregación: LAG y LACP (IEEE 802.3ad)\nConmutación por protección de anillos: ITU-T G.8032 ERPS.\nPropagación del estado del enlace\nJumbo tramas 16KB\nColas concientes configurables de QoS\n8 niveles de H-QoS con multiples opciones de mapeo:\nL2: 802.1p, VLAN id - L2½: MPLS EXP - L3: DSCP"]
[null,"1.13","Sincronización de tiempo","Synchronous Ethernet y 1588v2 TC"]
[null,"1.14","Seguridad","AES 128-bit y 256-bit (Se tiene que solicitar el HW)"]
[null,"1.15","Administración y aprovisionamiento","Configuración Zero-touch; administración In-band, out-of-band\nWeb GUI (configuración de un click de las unidades local y remota) & CLI\nembebido\nSNMPv2/3, TACACS+, RADIUS\nLink OAM & Connectivity Fault Management (CFM): IEEE802.3ah & IEEE802.1ag;\nMonitoreo: ITU-T Y.1731"]
[null,"1.16","Topologías","Anillo, daisy-chain, malla"]
[null,"1.17","Cumplimiento","Radio: FCC CFR Part 101, ETSI EN 302 217-2-2\nEMC: USA FCC 47CFR.part 15 & ETSI EN 301 489;\nSeguridad: UL/EN 60950"]
[null,"1.18","Alimentación","36÷57VDC; PoE In PoE++ (IEEE 802.3at+), 45W sin PoE-Out, 60W con PoE Out"]
[null,"1.19","PoE-Out","Puerto 2: hasta 13W (IEEE 802.3af)"]
[null,"1.20","Latencia","Latencia típica en mili-segundos"]
[null,"1.21","Ambiental","Temperatura de operación: -45° a +55°C (-49° a +131°F)\nProtección contra ingresos: IP67"]
[null,"1.22","Dimensiones","ODU + antena 0.5 pies (Dia. x Profundidad): 20 x 23 x 15cm (7.9” x 9” x 5.9”)\nODU + antena 1 pie (Dia. x Profundidad): 32 x 22 cm (12.6” x 8.6”)\nODU + antena 2 pies (Dia. x Profundidad): 73 x 46 cm (28.7” x 18.1” )"]
[null,"1.23","Peso","ODU + antena 0.5 pies: 3.8 kg (8.5 lbs)\nODU + antena 1 pie : 4.0 kg (8.8 lbs)\nODU + antena 2 pies: 9.4Kg (20.7lbs)"]
[null,2,"Estación Base"]
[null,"2.1","Marca","Especificar"]
[null,"2.2","Modelo","Especificar"]
[null,"2.3","Cantidad","De acuerdo al cuadro de cantidades"]
[null,"2.4","Tipo ","Radio Nodo Multihaul"]
[null,"2.5","Topologies","Point to Multi-point, Self-Backhaul L2 SDN Mesh\nPoint to Point"]
[null,"2.6","Sector(s)","Up to 4x 90° sector, for 360° coverage (license dependent).\nHorizontal scanning: 90°, per sector.\nVertical scanning: 50°"]
[null,"2.7","Frequency & Duplexing","57-66GHz.\nTDMA, Managed TDD, Terragraph certified."]
[null,"2.8","Channels & Width ","4x non-overlapping channels, 2160MHz wide. \nAny sector any of 4 channels, for optimal RF performance"]
[null,"2.9","Modulation & Coding","10 level of adaptive coding and modulation"]
[null,"2.10","Radio OTA Rate \n(over the air)","Up to 4600 Mbps"]
[null,"2.11","Aggregate Throughput","> 3800 Mbps per sector (license dependent)\n> 15Gbps per node"]
[null,"2.12","System Gain (link budget)","110dB (Node to Node/TU, including antenna gain)"]
[null,"2.13","Typical Reach \n(Node to Node/TU)","1000ft. (300m)"]
[null,"2.14","Interfaces","3 ports: 1x RJ-45 1/2.5/5/10GbE with PoE-In, 1x RJ-45 1GbE with PoE-Out (35W), 1x SFP+ \n10GbE"]
[null,"2.15","Ethernet Features","IEEE 802.1d transparent bridging.\nProvider bridge - VLAN & VLAN stacking."]
[null,"2.16","Security","GUI over HTTPS, CLI over SSH, AES 128-bits over the air"]
[null,"2.17","Management & \nProvisioning","In-band, Out-of-band management.\nWeb GUI (one-pane configuration of local and remote units) & Embedded CLI.\nNETCONF."]
[null,"2.18","Conformance","Radio: US FCC 47 CFR Part 15.255; EN 302 567.\nEMC: US FCC 47 CFR Part 15; EN 301 489;\nSafety: UL 62368."]
[null,"2.19","Power Supply","PoE, 55W no POE-Out, 90W with POE-Out (PoE-In: IEEE 802.3bt or passive; PoE-Out: IEEE \n802.3bt)"]
[null,"2.20","Environmental","Operating Temperature: -49° ÷ +131°F (-45° ÷ +55°C); Ingress Protection Rating: IP67"]
[null,"2.21","Dimensions","9.4 x 7 in. / 238 x 179 mm. (height x diameter)"]
[null,"2.22","Weight","8.8 lbs. (4 Kg)"]
[null,3,"Suscriptores"]
[null,"3.1","Marca","Especificar"]
[null,"3.2","Modelo","Especificar"]
[null,"3.3","Cantidad","De acuerdo al cuadro de cantidades"]
[null,"3.4","Tipo ","Unidad terminal Multihaul"]
[null,"3.5","Topologías","Punto a Punto, Punto a Multi Punto"]
[null,"3.6","Barrido de auto alineación","Escaneo horizontal: 90°.\nEscaneo vertical: 50°"]
[null,"3.7","Frecuencia y duplexado","57-66GHz, TDD/TDMA"]
[null,"3.8","Canales y ancho de canal","4x canales que no se empalman, 2160MHz por canal"]
[null,"3.9","Modulación y codificación","10 niveles de modulación y codificación adaptativa"]
[null,"3.10","Tasa de transferencia OTA\n(en el aire)","Hasta 4,600 Mbps"]
[null,"3.11","Ancho de banda","1000 Mbps."]
[null,"3.12","Alcance típico \n(Nodo a TU)","300m / 1000ft."]
[null,"3.13","Interfaces","T265-CCP, 3 puertos: 1x RJ5/2.5 con PoE-In, 1x RJ-45 1GbE con PoE-Out (35W), 1x SFP+ \n10GbE.\nT265-CNN, 1 puerto: 1x RJ-45 2.5/1GbE con PoE-In."]
[null,"3.14","Características Ethernet","Bridge IEEE 802.1d transparente,\nProvider bridge - VLAN y VLAN stacking"]
[null,"3.15","Seguridad","AES 128-bits OTA, GUI sobre HTTPS, CLI sobre SSH"]
[null,"3.16","Gestión y \naprovisionamiento","Gestión dentro y afuera de la banda,\nWeb GUI (configuración de unidades locales y remotas), CLI integrado y NETCONF"]
[null,"3.17","Cumplimiento","Radio: US FCC 47 CFR Part 15.255; EN 302 567,\nEMC: US FCC 47 CFR Part 15; EN 301 489,\nSeguridad: UL/IEC 62368-1; UL/IEC 60950-22"]
[null,"3.18","Energía"," PoE, 35W sin salida POE; 90W con salida de 65W POE-Out\nPoE-In: IEEE 802.3bt o pasivo; T265-CCP: PoE-Out: IEEE 802.3bt"]
[null,"3.19","Ambiental","Temperatura de operación: -45° ÷ +55°C (-49° ÷ +131°F); Protección de Entrada: IP67"]
[null,"3.20","Dimensiones","175 x 220 x 125 mm. / 6.9 x 8.6 x 4.9 in. (A x A x P)"]
[null,"3.21","Peso","2.2 Kg. / 4.84 lbs"]
[null,4,"Equipo de red"]
[null,"4.1","Marca","Especificar"]
[null,"4.2","Modelo","Especificar"]
[null,"4.3","Cantidad","De acuerdo al cuadro de cantidades"]
[null,"4.4","Tipo ","Router"]
[null,"4.5","CPU","TLR4-03680"]
[null,"4.6","CPU core count",36]
[null,"4.7","CPU nominal frequency","1.2 GHz"]
[null,"4.8","Dimensions","443 x 193 x 44 mm"]
[null,"4.9","Size of RAM","4 GB"]
[null,"4.10","Storage size","1 GB"]
[null,"4.11","Storage type","NAND"]
[null,"4.12","MTBF","Approximately 200'000 hours at 25C"]
[null,"4.13","Tested ambient temperature","(-)20C to 60°C"]
[null,"4.14","IPsec hardware acceleration"]
[null,"4.15","Number of AC inputs",2]
[null,"4.16","AC input range","100-240"]
[null,"4.17","Max power consumption","60W"]
[null,"4.18","FAN count",2]
[null,"4.19","10/100/1000 Ethernet ports",12]
[null,"4.20","SFP DDMI"]
[null,"4.21","SFP ports",4]
[null,"4.22","Serial console port","RJ45"]
[null,"4.23","Number of USB ports",1]
[null,"4.24","USB Power Reset"]
[null,"4.25","USB slot type","USB type A"]
[null,"4.26","Max USB current (A)",1]
[null,"4.27","Number of M.2 slots",1]
[null,"4.28","CPU temperature monitor"]
[null,"4.29","PCB temperature monitor"]
[null,"4.30","Voltage Monitor"]
[null,"4.31","Mode button"]
[null,"4.32","Certification","CE, EAC, ROHS"]
[null,"4.33","IP","IP20"]